
This manual describes FingerCell product activation on embedded platforms
=========================================================================

There are two possible activation scenarios, please choose the one suitable for You:

A scenario: You are using embedded device in stand-alone mode, i.e. You don't use 
any auxiliary software like ActiveSync to access Internet from Your device.

	1. Copy all essential files from the distribution to Your device: folder bin\ppc03_armv4\
	2. Enter "Activation\Device" directory
	3. Run the "pg" program, the application window should appear, with two buttons 
		"Exit" and "Help", the program should start without any messages,
		in case of error message, please contact support@neurotechnologija.com

	4. Click "X" to minimize the program
	5. Go to " bin\ppc03_armv4" directory 
	6. Run FncDemo.exe
	7. Try the Demo program

B scenario: You are using embedded device attached to Host computer through some wire of 
docked station and device is communicating with Your Host computer using ActiveSync or 
similar software.

	1. Enter "bin\ppc03_armv4\Activation\Host\" directory on Host computer and run "register.bat", 
		check if "Neurotechnologija" service is available in Your operating system 
		(control panel->administrative tools->services) after that. If no service 
		available, please contact support@neurotechnologija.com

	2. Copy all essential files to Your device: folder bin\ppc03_armv4\

	3. Copy the "pg.conf" file to Your handheld where "pg.exe" resides in bin\ppc03_armv4\Activation\Device\ foleder
	4. Edit the handheld's "pg.conf" file:
		a) chande "Mode = server" to "Mode = gateway"
		b) change "Address = 0.0.0.0" to "Address = HOST_IP", replace the HOST_IP with 
			LAN IP address of Your host computer, e.g. "Address = 192.168.0.11"
	5. Run the "pg" program, the application window should appear, with two buttons "Exit" and "Help",
		the program should start without any messages,
		in case of error message, please contact support@neurotechnologija.com

	6. Click "X" to minimize the program
	7. Go to " bin\ppc03_armv4" directory 
	8. Run FncDemo.exe
	9. Try the Demo program

NOTE: If You have some custom environment or these instructions doesn't meet You needs, or
	You have failed to complete some step, please contact us: support@neurotechnologija.com
